HLR Section 1.7
Limitations & Restrictions
Structure Data | Maximum number of spans in continuous bridges | 19
| Maximum number of spans in simply supported bridges | 100
| Maximum number of span groups | 11
| Maximum number of spans in a span group | 101
Route & Link Data | Maximum number of characters in a node number | 3
| Maximum number of characters in a route number | 8
Vehicle Data | Maximum number of axles in a vehicle | 99
Analysis | Maximum working overstress limit | 140%