# HLR - Main Index

Last updated 23 February 2001
1. Program Overview
1.1 | General procedure
1.2 | Analysis process
1.3 | Simply supported structures
1.4 | Continuous structures
2. Job Identification Data
2.1 | Names and descriptions
2.2 | HL and application numbers
2.3 | Retrieve an application from the Data Base
3. Route Data
3.1 | Overview
3.2 | Create new routes from links
3.3 | Create new routes using sections of existing routes
4. Vehicle Data
4.1 | Vehicle description data
4.2 | Axle and load data
4.3 | Retrieve a vehicle from the data base
5. Structure Data
5.1 | Structure identification data
5.2 | General structure data
5.3 | Span data
5.4 | Moment capacities
5.5 | K-Factors
5.6 | Shear and reaction capacities
6. Analysis
6.1 | Analysis options
6.2 | Moment capacity data is available for a structure
6.3 | Moment capacity data is not available (Ratio Method)
6.4 | K-Factor analysis
6.5 | Shear and reaction checks
6.6 | Checking NT single lane bridges
6.7 | Dynamic Load Allowance (DLA factor)
6.8 | Other checks
7. Reports & Results
7.1 | Reports and results
8. Defaults & Customisation
8.1 | General program defaults
8.2 | Directory paths
8.3 | Load effect factors
8.4 | Dynamic load allowance curve
8.5 | Phi factors
8.6 | Factors for Northern Territory single lane bridges
Top of page
| Please e-mail comments & suggestions to: George Sobol
| Structural & Geotechnical Section, TransportSA Ph: (08) 8343 2330 Fax: (08) 8343 2257